Warpzilla README

This README file contains the latest information about using
Warpzilla.


Note: To help you locate information in this README file, you can use
      the Find option under the Edit menu of the OS/2 System
      Editor. You can print the file by dragging it to your
      printer object, or by selecting Print from the file object's
      pop-up menu. Using the right mouse button, click the object
      to display the pop-up menu.

CONTENTS
________

1.0  RESTRICTIONS
2.0  LIMITATIONS
3.0  USING TCP/IP WITH WEB BROWSER
4.0  ENABLING THE LOOPBACK INTERFACE
5.0  CONFIGURING THE SOCKS SERVER CONNECTION
6.0  CONNECTING TO SECURE WEB SITES
7.0  USING AUTOMATIC PROXY CONFIGURATION
8.0  EXPORTING ADDRESS BOOKS FROM NETSCAPE(R) COMMUNICATOR
9.0  PRINTING
10.0 TRADEMARKS


1.0 RESTRICTIONS
________________

The following sections describe Warpzilla restrictions.


1.1 FAT (file allocation table) file system support
---------------------------------------------------
Because Warpzilla requires long file names, it cannot be installed 
on a FAT file system; however, you can install Warpzilla on a 
partition other than the partition where the operating system resides. 
For example, your operating system might reside on the C partition, 
which is a FAT partition, but you can install Warpzilla on the D 
partition, which is an HPFS (High Performance File System) partition.


1.2 Unsupported elements
------------------------
Warpzilla does not support the following:
- Dynamic Data Exchange (DDE)
- Netwatch
- HTML Publishing
- Smart Update
- Plug-in printing
- Lightweight Directory Access Protocol (LDAP)


2.0 LIMITATIONS
_______________

The following sections describe Warpzilla limitations.


2.1 Netscape 4.61 Plug-ins
--------------------------
To use Netscape 4.61 Plug-ins, copy the files from the 
NETSCAPE\PROGRAM\PLUGINS directory to the MOZILLA\PLUGINS 
directory.


2.2 Viewing Web pages
---------------------
Warpzilla adheres to the Internet standards set by WWW 
Communications (www.W3C.com). Web pages that do not 
comply with these standards might not display correctly.


2.3 Unicode Web pages
---------------------
Unicode Web pages do not display correctly.


3.0  USING TCP/IP WITH WEB BROWSER
_________________________________

If you have IBM TCP/IP Version 2.0 (see the SYSLEVEL.TCP entry 
in the SYSLEVEL output) and do not have CSD level UN64092 or 
higher installed, install CSD files level UN64092 or higher
(depending on which CSD level is available in the IBM FixPak 
Database).

If you have IBM OS/2 LAN Adapter and Protocol Support (see the
SYSLEVEL.TRP file in the SYSLEVEL output) and do not have CSD
level WR08210 or higher installed, install CSD files level
WR08210 or higher (depending on which CSD level is available
in the IBM FixPak Database).


4.0 ENABLING THE LOOPBACK INTERFACE
___________________________________

To visit secured Web sites with Warpzilla, you must enable the 
loopback interface in TCP/IP before you start Warpzilla. The 
loopback interface resides under the NETWORK tab of the TCP/IP 
configuration. Verify that Enable Interface is selected and that
the IP address is set to 127.0.0.1.

NOTE: When you use a modem to connect to the Internet, the loopback 
interface might become disabled. To enable the loopback interface 
after you connect to the Internet, type the following command at 
an OS/2 command prompt:

    ifconfig lo 127.0.0.1


5.0 CONFIGURING THE SOCKS SERVER CONNECTION
____________________________________________

To connect to a Web site through a SOCKS server, configure 
the SOCKS server connection at the system level, by specifying the 
SOCKS host address in the TCP/IP Configuration notebook. If you 
try to specify the SOCKS server address through Edit -> Preferences 
in Warpzilla, your secure connections will be refused.


6.0 CONNECTING TO SECURE WEB SITES
__________________________________

Warpzilla might stop loading a Web page while trying to 
connect to a secure Web site (without displaying an error 
message) because the server that you are connecting to has 
an incomplete implementation of TLS (Transport Layer 
Security). You might try to disable TLS in Warpzilla. 
To disable TLS:

1. Click the lock icon in the lower right corner of the Warpzilla window.
2. Click on the Advanced tab.
3. Click Options.
4. Uncheck Enable TLS.


7.0 USING AUTOMATIC PROXY CONFIGURATION
_______________________________________

To use Automatic Proxy Configuration, select Edit -> Preferences ->
Advanced -> Proxies. Then, select Automatic Proxy Configuration URL 
and type the appropriate URL in the text box.

NOTE: Warpzilla does not support SOCKS in the Automatic Proxy 
Configuration file.


9.0 EXPORTING ADDRESS BOOKS FROM NETSCAPE COMMUNICATOR
______________________________________________________

Because you cannot export address books from Netscape Communicator,
you cannot import address books from Netscape Communicator into 
Warpzilla.


9.0 PRINTING
____________

To set the number of copies you want to print, change the value 
in the printer device driver. If you encounter problems when you 
print, verify that you have the latest driver for your printer.


10.0  TRADEMARKS
__________________________________________________________________

The following terms, are registered trademarks of the IBM
Corporation in the United States or other countries or both:

  o IBM

  o OS/2

The following terms are trademarks of other companies:

Netscape is a registered trademark of Netscape Communications 
Corporation in the United States and other countries. 

Mozilla is a trademark of Netscape Communications Corporation in the 
United States and other countries.
